api5l3t                 API 5L. Values of SMYS and UTS
b31crvl                 ASME B31G. Basic computer program CRVL.BAS
b31gacd                 ASME B31G. Allowable corrosion depth in pipe
b31gacl                 ASME B31G. Allowable corrosion length in pipe
b31gafr                 ASME B31G. A-factor
b31gdata                ASME B31G. Corrosion state of 12 pipes
b31gdep                 ASME B31G. Design pressure of pipe
b31gmodpf               ASME B31G. Failure pressure of the corroded
                        pipe (modified)
b31gops                 ASME B31G. Operational status of pipe
b31gpf                  ASME B31G. Failure pressure of the corroded
                        pipe (original)
b31gsap                 ASME B31G. Safe maximum pressure for the
                        corroded area of pipe
c_k                     Convert to Celsius scale
dnvpf                   DNV-RP-F101. Failure pressure of the corroded
                        pipe
dropg                   Flow rate drop in pipe
dropp                   Pressure drop in pipe
dropt                   Temperature drop in cylindrical steel pipe due
                        heat loss
f_k                     Convert to Fahrenheit scale
flowls                  List all possible flow paths in district
                        heating network
fric_buzelli            Estimate pipe friction factor with Buzelli
                        formula
fric_romeo              Estimate pipe friction factor with Romeo's
                        formula
fric_vatankhan          Estimate pipe friction factor with Vatankhah
                        formula
geoarea                 Calculate geographical metrics
inch_mm                 Millimeters to inches
k_c                     Covert to Kelvin scale
kgf_mpa                 Megapascals to kilogram-force per square
loss_flux               Convert heat flux to specific heat loss power
m278hlair               Minenergo-278. Normative heat loss of open-air
                        pipe
m278hlcha               Minenergo-278. Normative heat loss of pipe in
                        channel
m278hlund               Minenergo-278. Normative heat loss of
                        underground pipe
m278insdata             Minenergo-278. Thermal conductivity terms of
                        pipe insulation materials
m278inshcm              Minenergo-278. Thermal conductivity of pipe
                        insulation materials
m278soildata            Minenergo-278. Thermal conductivity of subsoil
                        surrounding pipe
m325beta                Minenergo-325. Local heat loss coefficient
m325nhl                 Minenergo-325. Normative heat loss of pipe
m325nhldata             Minenergo-325. Normative heat loss data
m325testbench           Minenergo-325. Test bench of district heating
                        network
m325tracebw             Minenergo-325. Massively trace backwards
                        thermal-hydraulic regime for district heating
                        network
m325tracefw             Minenergo-325. Massively trace forwards
                        thermal-hydraulic regime for district heating
                        network
m325traceline           Minenergo-325. Trace thermal-hydraulic regime
                        for linear segment of district heating network
mepof                   Probability of failure of the corroded pipe
                        within maximum entropy
meteos                  Get list of weather stations (meteos)
mgtdhid                 Get ground temperature
mm_inch                 Inches to mm
mpa_kgf                 Kilogram-force per square cm to megapascals
mpa_psi                 Pounds per square inch to megapascals
pcorrcpf                PCORRC. Failure pressure of the corroded pipe
pipenostics-package     pipenostics: Diagnostics, Reliability and
                        Predictive Maintenance of Pipeline Systems
psi_mpa                 Megapascals to pounds per square inch
re_u                    Estimate Reynolds number
shell92pf               Shell92. Failure pressure of the corroded pipe
strderate               DNV-RP-F101. De-rate yield stress and tensile
                        strength of pipe due to temperature
tracebw                 Massively trace backwards thermal-hydraulic
                        regime for district heating network
tracefw                 Massively trace forwards thermal-hydraulic
                        regime for district heating network
traceline               Trace thermal-hydraulic regime for linear
                        segment of district heating network
wth_d                   Derive the wall thickness depending on the
                        outside diameter of pipe
